PLANET Voice over IP Product Firmware/Utility Release
---------------------------------------------------
Product supported: IPX-2500(v3)
Release date: 02/13/2019
New Release Version: v3.1.1

Added:
1. Added Meet Me Page feature
2. Added Call Duration limitation in the dial rules
3. Added Seize CO Line feature, by dialing the BLF number of the FXO port to seize the line and dial the phone number upon the dial tone
4. Added Time Condition support for the Direct Routing
5. Added IVR prompts recording through extension
6. Added Outbound CID option for the Dial Rules
7. Added dial 0 to reach the operator extension from voicemail
8. Added Permit IP option to the IP extensions
9. Added Language option to the IVR for selecting system voice prompts language
10. Added Dial by Name feature and added as an IVR event option
11. Added timeout option for call forward on no answer
12. Added contact sort for LDAP phonebook
13. Added Czech language support for both Web GUI and system voice prompts
14. Added high definition codec support for SIP trunks (amr and amrwb)

Fixed:
1. Fixed the issue of when Office Closed feature is enabled with call destination set as IVR which doesn't work
2. Fixed the issue of when Outbound Fax is enabled the Outbound CID will display as "null"
3. Fixed the issue of when extented voicemail is disabled, this extension cannot be selected while bulk adding DID number for direct routing
4. Fixed the issue of incorrect analog extension status, when analog extension number had been modified
5. Fixed the issue of non-authenticated trunk register status delay that got value 0.0ms
6. Improved inbound and outbound fax features
7. Fixed the issue of department ring group that would not divert calls to another department ring group after ring timeout
8. Fixed the issue of the third local network address that could not be added to the NAT settings
9. Fixed the issue of inbound route on SIP trunks
10. Adjusted default SIP TCP protocol port as 5060
11. Fixed the issue of dial rules that didn't work after creation
12. Fixed the issue of L2TP VPN server that would not start
13. Fixed the issue of inbound and outbound calls that would not work owing to incorrect analog line parameters
14. Fixed incorrect extension status in the early software versions


---------------------------------------------------
Product supported: IPX-2500(v3)
Release date: 10/31/2018
New Release Version: v3.0.3

Added:
1. Enhanced the function of IVR name dialing
2. Increased the ability of the phone to record IVR voice


Fixed:
1. Fixed the extension line that could not ring normally in the department.
2. Modified the phone to automatically configure the phone and click the "Activate" button after selecting the phone.
3. Fixed the issue of the DDNS program that could not be used.


----------------------------------------------------
Product supported: IPX-2500(v3)
Release date: 7/30/2018
New Release Version: v3.0.2


*** v3.0.2
1. Initial Release



Upgrade Method
===========
To upgrade the firmware of your IP PBX, please logon to your machine and click on the "System" menu. In the "System" menu, choose the "Update" page.
On this page, you click the Browse button to allocate the firmware file on your PC. Once the new firmware file is selected, click "Upload" to start the upgrade process. 
Please also check "Restore Default Set" after the update that will reset to the factory default setting.

Note:
=====
1. Do not turn the power off during the upgrade process. This will damage the unit.
2. Do not upload a different model's software. This will damage the unit.
3. File name must be "uImage-md5"; if the file name is changed, it will show "File name error". 
4. The version 2 firmware does not work with version 1 and version 2.



Thanks for choosing PLANET products.


Best Regards,


PLANET Tech SupportTeam

VoIP Technical Service: support_voip@planet.com.tw